Installation instructions
1. Follow Sections 1 and 2 of FPGA-UG-02229-1-0-FPGA-AI-Firmware-Pipeline-User-Guide.pdf using the Lattice sensAI FPGA AI Firmware/FPGA_AI_Firmware_HMI_v2.4ba601d.bin file as VVML NX33 board SPI Flash memory image binary.

Running the demo.
1. You can use EveVisualizer.exe available on this page https://www.latticesemi.com/en/Products/DesignSoftwareAndIP/AIML/Lattice-sensAI-Edge-Vision-Engine-SDK and follow the instructions in its User Guide at the section titled "CrossLink-NX-33 Integration".